Turn on and off hotspot

**Functional Description**

Users can choose to turn on or off the car hotspot according to their needs, with the default setting being off. Only when the vehicle is stopped can the hotspot be turned on or off by touching SWP. When the vehicle is in motion, hotspots can be turned on/off through voice.

Enabling conditions (a&b):

IVI system startup;

User can operate SWP.

Trigger conditions (a|b):

User operates the soft switch on the SWP to turn on/off the car's hot spot.

User wakes up the voice assistant and turns on/off the car's hotspot through voice commands.

The user wakes up the voice assistant and turns on/off the car's hotspot through voice commands.

Execution output (a & b):

IVI\_IFT sends vehicle/{VIN}/hardware/interfaces/hotspotCommand signal.

IVI\_IFT sends vehicle/{VIN}/hardware/interfaces/hotspotCommand signal.

IVI\_IFT receives hotspot status signal vehicle/{VIN}/hardware/interfaces/hotspotState

and displays hotspot status on the hotspot control page.

Exit conditions (a):

IVI system shutdown;