Switch music sources

**Functional Description**

Users can switch music sources through the SWP or voice. It can only be used when the vehicle is stopped through SWP operation.

Enabling conditions (a & b):

IVI system startup;

Users can operate the SWP.

Trigger conditions (a | b):

The user clicks on the SWP to select the corresponding audio source.

The user wakes up the voice assistant and switches the audio source through voice commands.

Execution output (a):

The system switches the corresponding audio source.

The system switches the corresponding audio source.

Exit conditions (a):

IVI system shutdown;

The SWP can switch between network/USB/Bluetooth music interfaces.

The voice recognition system can recognize audio source switching commands.

The SWP can switch between network/USB/Bluetooth music interfaces.

The voice recognition system can recognize audio source switching commands.